TURBOSOUND EASE FOCUS 3 GLL FILES FOR:
MV212 & MV212-XV  / MS215 using MAN-FG (also MS215 ground stack)'standard' V2.2

MS218 'standard' V1.6

MV210-HC / MS121 using MAN210-FG (also MS121 ground stack) 'standard'V1.9

MC12-P 'standard'V1.3

MS121 Cardioid Subwoofer Array V1.0
MS121 Subwoofer Array V1.3

MS215 Cardioid Subwoofer Array V1.0
MS215 Subwoofer Array V1.3

MS218 Cardioid Subwoofer Array V1.0
MS218 Subwoofer Array V1.4

All data is based on the Lake 'Manchester Rev2.1 XP' presets, no other data is supported.
Data is exactly as recorded by winMF no manipulation of FR/Phase has been made.


KNOWN BUGS/FAULTS/LIMITATIONS:


NOTE: 
Use 'line array gll' to create 'cardioid' cabinet to physically reverse cabinet then click filter settings to choose correct preset - 
these all relate exactly to the Lake 'Manchester Rev2.1 XP' presets

PLEASE USE EASE Focus 3 - Release Version 3.1.180
https://focus.afmg.eu/index.php/fc-downloads-en.html

RESOURCES
https://www.afmg.eu/en/resources     (add Ease Focus into drop down)

USER GUIDE
https://www.afmg.eu/en/ease-focus-3-users-guide

SUBARRAY PRESENTATION - VITAL READING FOR USING SUB ARRAYS!
https://www.afmg.eu/en/focus-your-sub-arrays

SW & HW Requirements
https://www.afmg.eu/en/ease-focus-software-hardware-requirements


Any bugs please report to: enterprisesolutions@musictribe.com




